**Container Checklist**

Container No. : Seal No. :

Exporter :

Importer :

**Front wall** – blocks and vents should be visible; use tool to tap front wall and listen and feel for hollow sound; use a range finder, measuring tape or string to determine the length of the container(see chart below for dimensions).

**Left side** – unusual repair to structural beams, use tool to tap side wall of container and listen and feel for hollow sound, repairs to the walls on the inside of the container must be visible on the outside.

**Right side** –unusual repair to structural beams, use tool to tap side wall of container and listen and feel for hollow sound, repairs to the walls on the inside of the container must be visible on the outside.

**Floo**r – floor should be certain height from ceiling (see chart below), floor should be flat, check for different floor heights within container; unusual repairs.

**Ceiling/Roof** – ceiling is certain height from floor (see chart below), blocks and vents are visible; repairs to the ceiling/on the inside of the container must be visible on the outside; use tool to tap side wall of container and listen and feel for hollow sound.

**Inside/Outside doors** – secure and reliable locking mechanism, look for different color bonding material, loose bolts, plates and repairs.

**Outside undercarriage** – support beams should be visible (use mirror to view underside)

**Confirm Container Dimensions:**

**20’ Standard Container 40’ Standard Container**

Inside Length : 5,919mm (19’5”) Inside Length : 1,2051mm (39’6.5”)

Inside Width : 2,340mm (7’8”) Inside Width : 2,340mm (7’8”)

Inside Height : 2,380mm (7’9.5”) Inside Height : 2,380mm (7’9.5”)

This is to certify, above check list performed and check marked properly. Finding any irregularities during inspection will be immediately reported to local law enforcement agency, respective carrier and forwarder. Hard copy of checklist will be kept in a file secure area for 180 days. A copy of checklist provided to forwarder immediately after merchandise being loaded and sealed for their record as required by C-TPAT Supply Chain.

Company Name :

Supervisor’s Name :

Signature : Date :

(Signature & Company Seal required)

**Note : Incomplete container check list/declaration will be subject to hold at terminal.**